*Wild Hair Accessories*Exclusive Motorcycle & StreetFighter Accessories

Mounting instructions GSG Peg Lowering Kit / Replacement Pegs

1. Rider Pegs: From the original pegs, remove the screw, bolt, nut, safety pin etc.
 Only for Yamaha Sport-Bikes: Remove Rivet, grind rivet head from underneath.

2. Remove bolt, pay attention to the way in which the spring is installed.

 If a spring is included, you must use the included spring.

 Original Distance pieces must be used. If they sit too tight, they must be pressed out.

 Peg Lowering Kit only
3. The pegs are adjustable in various steps on the bracket. Loosen the screw and adjust the
 bracket in to position. Make sure left and right side are in the same position.
 Torque for M8 Screws is 23 Nm.

4. Place the spring in position (as it was originally) install the peg with screw or bolt and tighten it.

5. Make sure you use the included washers and screws.
 Adjust the peg and tighten it with 9.5 Nm
6. Adjust levers

 Passenger pegs:

1. While you remove the passenger pegs, pay close attention to spring and metal ball.
 You will need to re-use them (often times the pressure causes them to pop out)
 Remember the position of the spring, metal ball if applicable, distance pieces etc.

 Install the passenger pegs in the reverse order.

2. Tighten all screws. Extension to adapter, peg to extension

 .

After the pegs are installed, use a little chain lubricant on the foldable joints.

Tip: Install one peg at a time. You still have a chance to check the other side on how it mounts.